Winlink Packet Radio Setup Notes
Updated 26 April 2020

MFJ TNC 2  (MFJ-127x)
•	Set as "TAPR TNC2" in Packet Winlink/P2P Setup
•	Baud rate is generally 9600
Icom 7200 / 9100 Radios, packet software
•	This YouTube video explains the software and setup for Winlink Express:
https://youtu.be/yBjV_9ayrVc
Software Packet-Radio TNC
•	http://uz7.ho.ua/packetradio.htm